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METALITE® STANDING SEAM FAÇADE (SSF) PANEL SYSTEM
A Prefinished, Prefabricated Single-Skin Aluminum Panel Barrier System
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Tremco CPG Inc.
3735 Green Road
Beachwood, OH 44122


INTRODUCTION
This manufacturer’s guide specification is intended for use by design and construction professionals in the development of project specifications.  By referring to the manufacturer’s “Notes to Specifier” in parentheses and bolded, the specifier may easily select the portions of the comprehensive guide specification which are pertinent to the project.  “Notes to Specifier” should then be deleted from the final specification document.  This guide specification follows the Construction Specification Institute’s MasterFormat and SectionFormat protocols.
It is prudent to place certain parts of the Dryvit Standing Seam Facade System Specification in other parts of the project’s total specification, such as sheathing, air and water-resistive barrier membrane, accessory materials, sealants and framing, as applicable.  The project design professional is responsible for verifying that project specifications are suitable for any project.  For assistance in preparing your specifications, please contact your Dryvit Distributor, your local Dryvit Technical Sales Representative, or Dryvit Technical Services.
WARNING
The Standing Seam Facade System is defined as a single-skin aluminum panel cladding barrier system. The barrier system is intended to block air and water infiltration from penetration of the outermost face of the barrier system. However, a tested and approved air and water-resistive barrier is recommended be installed over the exterior substrate to prevent water intrusion to the interior wall cavity or other interior building components.  Care should be taken to ensure that all building envelope elements, such as roofing, windows, flashings, sealants, etc., are compatible with the Metalite Standing Seam Facade System.
The Standing Seam Facade System is a prefabricated panel system of numerous compatible components such as roll-formed aluminum panels, click rails, and other accessories, and can include an approved air- and water-resistive barrier.
DISCLAIMER
It is the responsibility of both the specifier and the purchaser to determine if a product is suitable for its intended use.  The designer selected by the purchaser is responsible for all decisions pertaining to design, detail, structural capability, attachment, shop drawings, etc.  The single-skin aluminum panel system Manufacturer has prepared guidelines in the form of specifications, installation details, application instructions and product data sheets to facilitate the design process only.  The Manufacturer is not liable for any errors or omissions in design, detailing, structural capability, attachment, project-specific shop drawings, or the like, whether based upon the information prepared by the Manufacturer or otherwise, or for any changes which purchasers, specifiers, designers, or their appointed representatives may make to the Manufacturer’s published information.
The information contained in this specification conforms to standard detail and product recommendations for the installation of the Dryvit Standing Seam Facade System as of the date of publication of this document and is presented in good faith.  Tremco CPG Inc. (Dryvit) assumes no liability, expressed or implied, as to the architecture, engineering or construction of any project.  To ensure that you are using the latest, most complete information, contact your local Dryvit Technical Sales Representative, visit our website at https://www.dryvit.com/or contact Dryvit Engineering at:
Tremco CPG Inc.
3735 Green Road, Beachwood, OH 44122
(800) 556-7752
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[bookmark: _Toc235015942]GENERAL
[bookmark: _Toc235015943]SUMMARY
Provide a prefinished single-skin aluminum standing seam wall panel system that includes the following:
Coordinated inside corner, outside corner, sill, header, jamb, lap and base flashings.
Clips and fasteners as necessary to meet design criteria and ensure complete installation.
[bookmark: _Toc235015944]RELATED REQUIREMENTS
[Note to Specifier: Delete any sections below not relevant to this project and add others as required.]
1. 03 30 00	Cast-in-place Concrete
03 40 00	Pre-cast Concrete
04 20 00	Unit Masonry
05 40 00	Cold-formed Steel Framing
05 50 00	Metal Fabrications
06 11 00	Wood Framing
06 11 00	Engineered Framing Systems
[Note to Specifier: Engineered framing system components such as parapet nailers and rough opening buck framing are available from Prebuck LLC, a division of Tremco CPG Inc. Coordinated specification of these items can be incorporated into the overall Tremco CPG limited warranty.] 
06 16 00	Sheathing
07 27 00	Fluid-Applied Air Barriers
[Note to Specifier: This specification contains options for the fluid-applied air/water-resistive barrier system and accessory materials that are approved for use behind the Metalite Standing Seam Facade System. Coordinate with Section 07 27 00 as required where an air/water-resistive barrier system is selected for use as outlined below in Section 2.2.E.]
07 62 00	Sheet Metal Flashing and Trim
07 92 00	Joint Sealants
08 40 00	Entrances, Store Fronts, and Curtain Walls
08 50 00 	Windows

[bookmark: _Toc235015945]references
Aluminum Association
2020 Aluminum Design Guide
American Society of Civil Engineers (ASCE)
ASCE-7 Minimum Design Lods for Buildings and Other Structures
American Society of Testing and Materials (ASTM)
ASTM B209 Standard Specification for Aluminum and Aluminum-Alloy Sheet and Plate
[bookmark: _Toc235015946]ADMINISTRATIVE REQUIREMENTS
Pre-Construction Meetings
[Note to Specifier: The Standing Seam Facade System Warranty requires a pre-construction meeting consisting of representatives from the Manufacturer, Applicator, Owner, and Consultant (if applicable) prior to the installation of the Products.] 
2. Conduct pre-installation meeting to verify project requirements, substrate conditions, and manufacturer’s installation instructions.
1. [bookmark: _Toc235015947]SUBMITTALS
GENERAL: Submit listed submittals in accordance with Conditions of the Contract and Division 1 Submittal Procedures Section.
PRODUCT DATA: Submit manufacturer’s specifications, standard details, and installation manual.
SHOP DRAWINGS:
Show wall panel system with flashings and accessories in elevation; sections and details. Include metal thicknesses and finishes, panel lengths, joining details, anchorage details, flashings and special fabrication provisions for termination and penetrations.  Indicate relationships with adjacent and interfacing work. 
Do not proceed with manufacture of wall materials prior to review of shop drawings and field verification of all dimensions.
SAMPLES:
Submit sample of panel section, 12" long x full width panel, showing proposed metal thickness, finish and profile.
CALCULATIONS:
Submit engineering calculations defining cladding loads for all wall areas based on design criteria listed in section 1.2 of this specification.
Calculation shall clearly indicate structural support type, spacing requirements of structural supports by zone, and fastener requirements.
Calculate pullout, pullover, and shear strength of fasteners in accordance with test data published by the fastener manufacturer, utilizing applicable material safety factors.
WARRANTY:
Provide unexecuted specimen warranty documents as required in section 1.8.
CERTIFICATION:
Submit manufacturer’s certification that materials and finishes meet specification requirements.
Submit applicator’s certification that installer of products meets specified qualifications Submit product data as required by Section 01 33 00, Administrative Requirements.
[bookmark: _Toc235015948]QUALITY ASSURANCE
MANUFACTURER’S QUALIFICATIONS:
Panel manufacturers must provide full supporting literature, flashing and details guides, Guide Specifications, and technical support.
INSTALLER QUALIFICATIONS:
Installer must have experience with at least 10 similar sized aluminum panel system projects in the past five (5) years.
Installer must be an approved installer, certified by the manufacturer prior to beginning installation of the wall.
PRODUCT SUBSTITUTION:
Products listed in this specification section are as manufactured by Tremco CPG, Inc.
Alternate wall panels will only be accepted with prior written approval of Architect.  
Substitution requests must be submitted in writing minimum ten days prior to bid date accompanied by product literature, technical information, and product sample. Approved substitutions will be set forth in an addendum.
No substitutions will be permitted after bid date.
[bookmark: _Toc235015949]DELIVERY, STORAGE, AND HANDLING
DELIVERY:
Deliver metal wall system to jobsite properly packaged to provide protection against transportation damage
HANDLING:
Exercise extreme care in unloading, storing, and erecting metal wall system to prevent bending, warping, twisting, and surface damage.
STORAGE AND PROTECTION:
store sheet bundles above ground with one end elevated and allow for air circulation and drainage.
Store sheet bundles under tarpaulin cover to protect from rain and prevent accumulation of dirt and condensation.
Prolonged storage of bundled sheets is not recommended.
ALWAYS avoid direct contact with alkali-bearing material such as lime-based cement, concrete/mortar. 
[bookmark: _Toc235015950]WARRANTY
Project Warranty: Refer to Conditions of the Contract for project specific warranty provisions.
Furnish Manufacturer’s standard 20-year warranty stating panel material will not fail due to:
Corrosion
Rupture
Perforation
Air/Water-Resistive Barrier Warranty:
[Note to Specifier: When the Metalite Standing Seam Facade panel system is installed over a Tremco CPG Inc. air/water-resistive barrier (AWRB), the selected AWRB warranty can be extended as follows:
[10-years] when Metalite Standing Seam Facade is installed over ExoAir 110AT or 210AT adhered air/water-resistive barrier membrane system. Coordinate with related Section 07 27 00.
[15-years] when Metalite Standing Seam Facade is installed over ExoAir 130 or 230 as the air/water-resistive barrier membrane system. Coordinate with related Section 07 27 00.
[20-years] when Metalite Standing Seam Facade is installed over Securock ExoAir 430 gypsum sheathing with factory fluid applied air/water-resistive barrier membrane system. Coordinate with related Section 06 16 00 and 07 27 00.
Installer’s Warranty: In a form acceptable to the Owner, Installer agrees to repair or replace metal wall panel assemblies that fail in materials and workmanship within two (2) years from date of Substantial Completion.
[bookmark: _Toc235015951]PRODUCTS
[bookmark: _Toc235015952]MANUFACTURERS
Tremco CPG Inc. (Dryvit), 3735 Green Road Beachwood, OH 44122, www.tremcocpg.com, www.dryvit.com, (800) 556-7752.
SUBSTITUTIONS:
Substitutions must fully comply with specified requirements.
Refer to specification Section 01630 - Product Options and Substitutions for substitution request procedures.
[bookmark: _Toc235015953]DESCRIPTION
SYSTEM DESCRIPTION
DESIGN REQUIREMENTS:
Design criteria shall be in accordance with current edition of the locally adopted Building Code.
Wall Loads:
Wall loads shall be as shown on the contract drawings or calculated per Building Code components/cladding criteria.  The largest inward/outward pressures (contract drawing specified or Building Code calculated) shall govern.
Deflection:
Wall panels shall withstand test pressures of inward and outward wind-load design pressures with maximum deflection of L/120 of the span.
STRUCTURAL REQUIREMENTS:
Panel structural properties are to be determined in accordance with latest edition of Aluminum Association’s “2020 Aluminum Design Manual- Specifications and Guidelines for Aluminum Structures”.
MATERIALS
Aluminum alloy sheet, ASTM B209, aluminum alloy 3004 or 3005 in accord with manufacturer’s standard to suit forming operations and finish specified Thickness: 0.031” to 0.047” (0.8mm-1.2mm).
Fabricated vertical leg standing seam panel with integral continuous overlapping seams suitable for continuous zipping or crimping by mechanical means during installation.
Panel seam shall allow for mechanical “unzipping” without compromise of panel structural integrity
Panels shall be 12" (305mm) / 13.1” (333mm) / 15.6” (400mm) / 16.9” (429mm) / 19.7” (500mm) with a vertical standing rib height of 2.0” (50mm) / 2.5” (65mm).
Acceptable Wall System: 
Metalite SSF-12 (12” wide, 2.5” tall) by Tremco CPG, Inc.
Metalite SSF-13 (13.1” wide, 2.5” tall) by Tremco CPG, Inc.
Metalite SSF-16 (15.6” wide, 2.5” tall) by Tremco CPG, Inc.
Metalite SSF-17 (16.9” wide, 2.0” tall) by Tremco CPG, Inc.
Metalite SSF-20 (19.7” wide, 2.5” tall) by Tremco CPG, Inc.
CLIP/FASTENER ASSEMBLIES:
“ST” Clip.  0.09” min. thickness extruded aluminum clip designed to freely accommodate thermal movement for panel lengths up to 130 ft.
“E” Clip.  One piece reinforced polyamide clip designed to freely accommodate thermal movement for panel lengths up to and beyond 130 ft.
ACCESSORIES:
Provide manufacturer’s standard accessories and other items essential to completeness of   standing seam wall panel installation.


AIR AND WATER-RESISTIVE BARRIER
[Note to Specifier: Select air/water-resistive barrier material as required for both the design intent and warranty requirements of Section 1.8 herein. Delete the remaining options below that are not applicable once selected for the Project.]
0. Permeable
Tremco ExoAir® 210AT: A permeable, self-adhered sheet designed to be applied to exterior cavity walls to mitigate air infiltration/exfiltration and water penetration while remaining permeable to the passage of water vapor. ExoAir 210AT can be installed in ambient air and substrate surface temperatures of 20°F (-6°C) and rising. The material shall be protected from rain and washout prior to drying and can be exposed for up to 12 months during the construction process.
Tremco ExoAir® 230/230LT: A thick-film synthetic, permeable, elastomeric air/water-resistive membrane barrier designed to be roller or spray applied. ExoAir 230 can be installed in ambient air and substrate surface temperatures of 40°F (5°C) and rising. ExoAir 230LT is a low-temperature grade of ExoAir 230 and can be installed in ambient air and substrate surface temperatures of 20°F (-6°C) and rising. The material shall be protected from rain and washout prior to drying and can be exposed for up to 12 months during the construction process.
Tremco Securock ExoAir® 430: USG Ultralight glass mat exterior sheathing, available in ½” or 5/8” Type X (UL Type USGX), with a factory-applied, high-performance air/water-resistive barrier coating. In-plant application of the membrane ensures uniformity, strong adhesion, climate independence during application, and eliminates in-field sheathing preparation. Joint and fastener detailing must utilize either Tremco Dymonic 100 sealant or ExoAir Dual Flash liquid flashing. Securock ExoAir 430 can be exposed for up to 12 months during the construction process.
Impermeable:
Tremco ExoAir® 110AT: An impermeable self-adhered sheet designed to be applied to exterior cavity walls to mitigate air infiltration/exfiltration, vapor transmission, and water penetration.  ExoAir 110AT can be installed in ambient air and substrate surface temperatures of 20°F (-6°C) and rising. The material shall be protected from rain and washout prior to drying and can be exposed for up to 12 months during the construction process.
Tremco ExoAir® 130: A thick-film synthetic, permeable, elastomeric air/water-resistive membrane barrier designed to be roller or spray applied.  ExoAir 130 can be installed in ambient air and substrate surface temperatures of 40°F (5°C) and rising. The material shall be protected from rain and washout prior to drying and can be exposed for up to 12 months during the construction process.


MISCELLANEOUS MATERIALS
FASTENERS:
All self-tapping/self-drilling fasteners and rivets shall be designed to withstand specified design loads.
All fasteners to be manufactured from series 304 austenitic stainless steel.  Rivet style fasteners to be manufactured from aluminum or stainless steel.
Provide neoprene washers under the heads of all exposed fasteners.
Use proper torque settings to obtain controlled uniform compression for a positive seal without rupturing the neoprene washer.
ACCESSORIES:
Provide all components required per the approved shop drawings for a complete metal wall system to include panels, fasteners, trims/flashings, extrusions and any other required items.
[bookmark: _Toc235015954]FABRICATION
PANELS:
Provide factory formed panels of the sizes listed below:
12.0" (305mm) wide with 2.5" (65mm) high standing seam
13.1” (333mm) wide with 2.5” (65mm) high standing seam
15.6” (400mm) wide with 2.5” (65mm) high standing seam
16.9” (429mm) wide with 2.0” (50mm) high standing seam
19.7” (500mm) wide with 2.5” (65mm) high standing seam
TRIM/FLASHING:
Fabricated trims/flashings to be from same material and gauge as wall panel system.
Fabricate trims/flashings in accordance with approved shop drawings and applicable standards.
[bookmark: _Toc235015955]FINISH 
NATURAL ALUMINUM:
Stucco Embossed.  Aluminum AA3004/3005 post processed through embossing rollers.
Natural Mill.  Aluminum AA3004/3005
PAINTED ALUMINUM:
Two-Coat Fluoropolymer Finish: Standard fluoropolymer 2-coat system consisting of 0.2 mil primer and 0.8 mil 70 percent PVDF fluoropolymer color coat.
Color: As selected from manufacturer’s standard colors
Color: As selected from manufacturer’s custom colors
Color: _________________.
Two-Coat Fluoropolymer Finish: MICA metallic appearing coating, 0.25 mil primer with 0.8 mil 70 percent PFCF fluoropolymer color coat containing pearlescent flakes.
Color: As selected from manufacturer’s standard colors
Color: As selected from manufacturer’s custom colors
Color: _________________.
Three-Coat Fluoropolymer Finish: Metallic finish, 0.25 mil primer with 0.75 mil 70 percent PVDF fluoropolymer coating containing metallic flakes and 0.5 mil 70 percent PVDF fluoropolymer clear top coat 
Color: As selected from manufacturer’s standard colors
Color: As selected from manufacturer’s custom colors
Color: _________________.
PRE-WEATHERED:
AluPlus Patina.  Smooth or stucco embossed aluminum substrate treated to provide weathered/matt appearance. 
ZINC COATED:
AluPlusZinc.  Aluminum substrate electrolytically fused with a 4 mm zinc layer on each side of sheet

[bookmark: _Toc235015956]EXECUTION
[bookmark: _Toc235015957]EXAMINATION
Examine the alignment and placement of the building structure and substrate. Correct any objectionable warp, waves or buckles in the substrate before proceeding with installation of the pre-formed metal wall panel.  The installed wall panels will follow the contour of the structure and may appear irregular if not corrected.
Do not proceed with installation until discrepancies have been resolved.
[bookmark: _Toc235015958]INSTALLATION
Install wall panels and flashings in accordance with approved shop drawings and manufacturer's product data, within specified erection tolerances.
Anchor panels securely in place using fasteners and spacing in accordance with manufacturer’s recommendations.
Do not allow panels or trim to come in contact with dissimilar materials such as copper, fire retardant treated timber, concrete/mortar.  Water runoff from dissimilar materials is also prohibited
[bookmark: _Toc235015959]

CLEANING
Clean exposed surfaces of excess material and debris promptly after completion of installation.
Clean installed products in accordance with manufacturer's instructions prior to owner's acceptance.
[bookmark: _Toc235015960]PROTECTION
Protect work as required to ensure wall panel system will be without damage at time of final completion.
Replace products having damage other than minor finish damage.
Repair products having minor damage to finish in accordance with panel manufacturer’s recommendations.

END OF SECTION
Issued 07/22/2026
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